For the connections, you will need to connect the following:  
  
For the JSN-SR04T sensor:  
  
VCC to 5V  
GND to GND  
TRIGGER to Pin 13  
ECHO to Pin 12  
For the ILI[9225](tel:9225) LCD:  
  
CS to Pin 15  
RST to -1 (not connected)  
DC to Pin 2  
MOSI to Pin 23  
CLK to Pin 18  
Please note that the connections may vary depending on the specific models of your components. Be sure to double-check the pinout diagrams for your specific models before making any connections.