wiring the LCD with Arduino is pretty easy

CS-A5

RST-A4

RS-A3

SDA-A2

CLK-A1

VCC- 5V

GND-GND