Here's the connection for the previous code again, with the added connection for the TFT LCD display:  
  
markdown  
Copy code  
JSN-SR04T     ESP32  
---------------------------------  
VCC           5V  
GND           GND  
Trig          GPIO4  
Echo          GPIO5  
  
LCD TFT        ESP32  
---------------------------------  
LED+          [3.3](tel:3.3)V  
LED-          GND  
SCK           GPIO18  
SDA           GPIO23  
A0            GPIO26  
RESET         GPIO27  
CS            GPIO14  
GND           GND  
VCC           [3.3](tel:3.3)V  
Again, make sure to double-check the pinout and connections for your specific TFT LCD display before connecting it to the ESP32